| Bill of Materials
Schematic: BeeLight Variant: PRELIMINARY Revision: + (Unreleased) Date: 2025-06-05 KiCad Version: 9.0.7+1 | Component Groups: 15 Component Count: 20 (per PCB) Fitted Components: 20 (per PCB) Number of PCBs: 1 Total Components: 20 (for 1 PCBs)

## Component Groups

Row | Quantity Per PCB | References | Value | Datasheet | Footprint | Description | manf | manf#
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 1 | BT101 | Battery_Cell | https://www.mouser.de/datasheet/3/201/1/3039.pdf | 3039 | Single-cell battery | Keystone | 3039
2 | 1 | C103 | 1n | https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C2A102JE02-01A.pdf | C_0402_1005Metric_Pad0.74x0.62mm_HandSolder | Unpolarized capacitor | Murata Electronics | GCM1555C2A102JE02D
3 | 5 | C101 C102 C104 C105 C106 | 100n | https://www.mouser.de/datasheet/2/40/KGM_X7R-3223212.pdf | C_0402_1005Metric_Pad0.74x0.62mm_HandSolder |  | KYOCERA AVX | 04025C104KAT4A
4 | 1 | D101 | IDENTIFY | https://www.mouser.de/datasheet/2/678/hsmq_c170_t0000_ds100-2498198.pdf | LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder | Light emitting diode | Broadcom / Avago | HSMQ-C170-T0000
5 | 1 | IC102 | APDS-9306-065 | https://docs.broadcom.com/docs/AV02-4755EN | Broadcom_DFN-6_2x2mm_P0.65mm |  | Broadcom / Avago | APDS-9306-065
6 | 1 | IC103 | BME688 | https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bme688-ds000.pdf | Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering | 4-in-1 sensor, gas, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8 | Bosch | BME688
7 | 1 | M101 | BL54L15 | https://www.ezurio.com/documentation/datasheet-bl54l15-series | BL54L15 | nRFL15 module | Ezurio | 453-00001C
8 | 1 | Q101 | BSS84 | https://www.mouser.de/datasheet/2/308/1/BSS84_D-2310226.pdf | SOT-23-3 | -0.13A Id, -50V Vds, P-Channel MOSFET, SOT-23 | onsemi / Fairchild | BSS84
9 | 1 | R102 | 0R | https://www.mouser.de/datasheet/2/54/cr_a_as-1858644.pdf | R_0805_2012Metric_Pad1.20x1.40mm_HandSolder | Resistor | Bourns | CR0805AJ/-000EAS
10 | 1 | R103 | 220R | https://www.mouser.de/datasheet/2/54/cr-1858361.pdf | R_0402_1005Metric_Pad0.72x0.64mm_HandSolder | Resistor | Bourns | CR0402-JW-221GLF
11 | 2 | R104 R105 | 1k8 | https://www.mouser.de/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf | R_0402_1005Metric_Pad0.72x0.64mm_HandSolder | Resistor | YAGEO | RC0402FR-071K8L
12 | 1 | R109 | 2k2 | https://www.mouser.de/datasheet/2/447/PYu_RT_1_to_0_01_RoHS_L_15-3461507.pdf | R_0402_1005Metric_Pad0.72x0.64mm_HandSolder | Resistor 62.5 mW 0.1 | YAGEO | RT0402BRD072K2L
13 | 1 | R108 | 8k2 | https://www.mouser.de/datasheet/2/447/PYu_RT_1_to_0_01_RoHS_L_15-3461507.pdf | R_0402_1005Metric_Pad0.72x0.64mm_HandSolder | Resistor 62.5 mW 0.1% | Yageo | RT0402BRD078K2L
14 | 1 | R101 | 100k | https://www.mouser.de/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf | R_0402_1005Metric_Pad0.72x0.64mm_HandSolder | Resistor | YAGEO | RC0402FR-07100KL
15 | 1 | SW101 | JOIN | https://www.we-online.com/components/products/datasheet/430182130816.pdf | WS-TASV-6x6 | Push button switch, generic, two pins | Wurth Elektronik | 430182095816

Color reference for columns:
KiCad Fields (default)
Generated Fields
User Fields
Empty Fields